#

##

##

##

##

##

##

    礦ision Build Log
    Tool Versions:
    IDE-Version: μVision V5.28.0.0
    Copyright (C) 2019 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: guangsen a, a, LIC=----

    Tool Versions:
    Toolchain:       MDK-Lite  Version: 5.28.0.0
    Toolchain Path:  D:\keil\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 6 (build 750)
    Assembler:       Armasm.exe V5.06 update 6 (build 750)
    Linker/Locator:  ArmLink.exe V5.06 update 6 (build 750)
    Library Manager: ArmAr.exe V5.06 update 6 (build 750)
    Hex Converter:   FromElf.exe V5.06 update 6 (build 750)
    CPU DLL:         SARMCM3.DLL V5.28.0.0
    Dialog DLL:      DARMCM1.DLL V1.19.2.0
    Target DLL:      CMSIS_AGDI.dll V1.31.18.0
    Dialog DLL:      TARMCM1.DLL V1.14.1.0

    Project:
    D:\李广森\work\pt068\开发包\PY32T020系列开发包 V1.3.3\PY32T020触摸开发资料 V1.3.3\1、Touch Library\PY32T020_Touch_Library_V1.3.3\Project\MDK-ARM\Py32t020xx_Touch.uvprojx
    Project File Date:  09/26/2024

    Output:
    *** Using Compiler 'V5.06 update 6 (build 750)', folder: 'D:\keil\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'PY32T020'
    assembling startup_py32t020xx.s...
    compiling system_py32t020.c...
    compiling main.c...
    compiling user_code.c...
    compiling uart_task.c...
    compiling drivers.c...
    compiling smg_task.c...
    compiling uart_drivers.c...
    compiling led_task.c...
    compiling adc_task.c...
    compiling gpio.c...
    compiling argb_task.c...
    compiling i2c_slave.c...
    compiling tim14_drivers.c...
    compiling tim1_drivers.c...
    compiling rtc_drivers.c...
    compiling led_drivers.c...
    compiling beep_drivers.c...
    compiling smg_drivers.c...
    compiling tm1624.c...
    compiling adc_drivers.c...
    compiling tm1640.c...
    compiling ir_received.c...
    compiling spi-led_drivers.c...
    compiling py32t020_ll_exti.c...
    compiling py32t020_ll_comp.c...
    compiling py32t020_ll_crc.c...
    compiling py32t020_ll_pwr.c...
    compiling py32t020_ll_gpio.c...
    compiling py32t020_ll_adc.c...
    compiling py32t020_ll_i2c.c...
    compiling py32t020_ll_rcc.c...
    compiling user-otp_drivers.c...
    compiling py32_flash.c...
    compiling py32t020_ll_spi.c...
    compiling py32t020_ll_rtc.c...
    compiling py32t020_ll_utils.c...
    compiling py32t020_ll_uart.c...
    compiling py32t020_ll_tim.c...
    compiling tk_user.c...
    linking...
    Program Size: Code=7740 RO-data=944 RW-data=140 ZI-data=1164
    FromELF: creating hex file...
    ".\Output\Py32t020xx_Library.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.5.5.1.pack
                    ARM.CMSIS.5.5.1
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 5.2.0

    Package Vendor: Puya
                    https://www.puyasemi.com/uploadfiles/Puya.PY32T0xx_DFP.0.0.6.pack
                    Puya.PY32T0xx_DFP.0.0.6
                    Puya PY32T0 Series Device Support

    Collection of Component include folders:
      .\RTE\_PY32T020
      D:\keill\Arm\Packs\ARM\CMSIS\5.5.1\CMSIS\Core\Include
      D:\keill\Arm\Packs\Puya\PY32T0xx_DFP\0.0.6\Drivers\CMSIS\Device\PY\PY32T0xx\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:5.2.0
    Build Time Elapsed:  00:00:10