================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了I2C通过轮询方式进行通讯，主机先向从机发送15byte数据，然后再接收从机
发送的15byte数据,主机、从机接收数据成功后，主机和从机板上的小灯处于“常亮”状态。

Function descriptions:
This sample demonstrates I2C communication using polling. The master sends 15 
bytes ofdata to the slave, and then receives 15 bytes of data from the slave. 
After successful data transmission and reception between the master and slave, 
the LEDs on both the master and slave boards will remain constantly lit.
================================================================================
测试环境：
测试用板：PY32MD320_STK
MDK版本： 5.28
IAR版本： 9.20
GCC版本： GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32MD320_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 先复位从机，然后再复位主机；
3. 复位完成后，按下主机user按键，主从开始通讯；
4. 观察主从机的LED灯，当主机和从机LED灯由常暗转为常亮状态，则表明主机、从机收发数
据成功；当主机或从机LED灯处于闪烁状态，则表明主机、从机收发数据失败。

Example execution steps:
1.Compile and download the program to the MCU and run it.
2.Reset the slave first, then reset the master.
3.After the reset is complete, press the user button on the master to start 
the communication between the master and slave.
4.Observe the LEDs on the master and slave boards. When the LEDs on both the 
master and slave boards change from being constantly dim to constantly lit, 
it indicates successful data transmission and reception between the master 
and slave. If the LEDs on the master or slave are blinking, it means that 
there was a failure in data transmission or reception.
================================================================================
注意事项：
PA9     ------> I2C_SCL
PA10    ------> I2C_SDA 
主机程序为I2C_TwoBoard_CommunicationMaster_Polling_Init
从机程序为I2C_TwoBoard_CommunicationSlave_IT_Init
如需修改速率，直接修改I2C_SPEEDCLOCK即可

Notes:
PA9 ------> I2C_SCL
PA10 ------> I2C_SDA
Master program: I2C_TwoBoard_CommunicationMaster_Polling_Init
Slave program: I2C_TwoBoard_CommunicationSlave_IT_Init
To modify the speed, simply modify the I2C_SPEEDCLOCK value.
================================================================================