================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了ADC模块的Tempsensor功能，并通过串口打印出温度值。

Function descriptions:
This example demonstrates the Tempsensor function of the ADC module and prints 
the temperature value through the serial port.
================================================================================
测试环境：
测试用板：PY32F403_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F403_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 串口每隔1s打印一次采集到的温度值。

Example execution steps:
1. Compile and download the program and run it;
2. The serial port prints the collected temperature values every 1 second
================================================================================
注意事项：
请检查芯片的高温校准值，如果是85，选择HighTemp_85，如果是105，选择HighTemp_105

通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下；
@PrintfConfigStart
STK板        USB转TTL模块
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

Notes:
Please check the high temperature calibration value of the chip. If it is 85, 
select HighTemp_85. If it is 105, select HighTemp_105

Connect the PC to the STK board through the USB to TTL module, and the connection
method between the STK board and the USB to TTL module is as follows:
@PrintfConfigStart
STK board USB to TTL module
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd
================================================================================